**Array of led circuitry**

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **S. No.** | **Components** | **Value** | **No. of components** | **Device** | **Library** | **Sub-library** | **Package** |
| 1 | LED | ------------ | 8 | Through hole | led | LED3MM (LED) | LED3MM |
| 3 | Resistor | 330E | 1 | Through hole | resistor | R-US | 0204/7 |

**Jumper/Connector:**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **S. No.** | **Jumper** | **No. of pins** | **No. of Jumper** | **Library** | **Sub-library** | **Package** |
| 1 | Jumper 1 | 8 | 1 | con-amp-quick | M08 | 08P |